Electrical

|  |  |  |
| --- | --- | --- |
|  | Motor M1 | Motor M2 |
| Connection | CH1@deviceX | CH2@deviceX |
| Current | 2 | 2 |
| Voltage | 24 | 24 |
| Micro Step | 64 | 64 |
| Encoder Line | 1024 | 1024 |
| POS | RISE | RISE |
|  |  |  |
| Lead | 60mm/r | 60mm/r |
|  |  |  |